Nitrogen Calibration Instructions

1. Hook up sensor to Arduino as listed in the schematic.
2. Place sensor inside the bag and seal behind.
3. Fill bag with 100% nitrogen, letting the bag leak and fill, till there is nothing but nitrogen in the bag.
4. Turn on the Arduino with Nitrogen Calibration Code.
5. Run it for 5 minutes.
6. Turn off Arduino.
7. Unplug sensor from circuit.
8. Upload the incubator Code to the Arduino.
9. Turn off Arduino.
10. Plug sensor back in, turn Arduino back on
11. Confirm the screen is reading the C02 level in the room.
12. Assemble Incubator
13. The sensor is now calibrated.